Scheme name=AWIPS color style

DIGITAL ATMOSPHERE  Color Tables  Edition 2
- Manual correction of this table is done at your own risk.
- Numerical values MUST always be zero-filled or space padded!
- Do not adjust column positions; they are fixed.
- Do not delete horizontal bar that begins the data section
- "Parameter name" can be anything you like - this is ignored by program
- OTHR/MISC has the following meanings:
    plf,plc/Station Plots = Default station crowding value (pixel radius, 0=no filtering)
- Font name: to manually override the font to Bold or Italic, add BOLD or ITALIC (capitalized)
    in the font name

                                COLOR VALUE  LN LINE  OTHR __FONT__
PRM  PARAMETER NAME             rrr-ggg-bbb  WD STYLE MISC SZ NAME
---------------------------------------------------------------------------------------------
bas  Background color           000-000-000  -                
lan  Land color                 000-000-000  -                
inl  International Boundary     200-200-170  2                
sta  State-Province Boundary    200-200-170  1        1       
cst  Coastline                  200-200-170  2                
isl  Islands                    200-200-170  2                
lak  Lakes                      200-200-170  2                
laf  Lake fill color            000-000-000                   
riv  Rivers                     200-200-170  2                
cty  Cities                     230-100-100  1  solid      8  Arial
lat  Lat/long graticule         050-050-050  1  solid         
shp  Shapefile data             080-080-120  1             8  Arial
leg  Legend block               220-220-220                10 System
stm  Map time stamp             255-255-128                8  Lucida Console
stb  Map time stamp background  000-000-000                   
plt  General plot color         200-200-200  1  solid      9  Wx Plot 7
plf  Station plots              255-040-046           15   9  Wx Plot 7
plc  Custom plots               255-255-255           25   10 Arial
pla  AMDAR plots                240-240-240                10 Arial
tdv  Television plot value      180-000-000  1             20 Arial
tdc  Television plot city       180-000-000  1             10 Arial
dy1  Convective Outlook Day 1   180-000-000  1                
dy2  Convective Outlook Day 2   180-000-000  1                
frc  Cold Fronts                000-000-240  2                
frw  Warm Fronts                240-000-000  2                
fro  Occluded Fronts            210-000-210  2                
frs  Stationary Fronts          000-000-000  2                
frt  Troughs                    250-183-154  3                
iso  General isopleths/labels   000-182-191  2             10 Arial
low  Low Pressure areas         240-000-000                30 Arial
hgh  High Pressure areas        000-000-240                30 Arial
max  Maxima                     000-000-160                20 Arial
min  Minima                     160-000-000                20 Arial
hw1  Highways                   240-230-210  2                
hw2  Highways                   230-230-090  2                
cnt  Counties                   240-190-120  1             6  Arial
cus  Custom geography           240-240-200                10 Arial
stl  Station reference lines    180-100-010  3                
stt  Station reference text     180-100-010                9  Arial
rad  NEXRAD general draw color  255-255-255                   
raf  NEXRAD legend font         255-255-020                10 Lucida Console
rab  NEXRAD legend background   000-000-000                   
ras  NEXRAD scale font          120-120-255                10 Lucida Console
rac  NEXRAD text annotations    000-000-150                10 Arial
rah  NEXRAD hail symbols        180-000-000                   
ral  NEXRAD hollow hail fill    240-240-240                   
ram  NEXRAD mesocyclone         200-000-000                   
rat  NEXRAD TVS                 220-000-000                   
rak  NEXRAD storm tracking      070-070-000                   
sfc  Lightning current          230-000-000                   
sfo  Lightning noncurrent       040-040-040                   
acu  Convective Outlook labels  255-255-255                10 Lucida Console
acg  Convective Outlook GEN     128-128-128  3  solid         
acs  Convective Outlook SLGT    000-180-000  3  solid         
acm  Convective Outlook MDT     180-180-000  3  solid         
ach  Convective Outlook HIGH    220-000-200  3  solid         
aca  Convective Outlook APCHG   064-128-128  3  solid         
acv  Convective Outlook SVR     000-200-000  3  solid         
ptt  Geographical Points        140-000-000  2             14 Arial
skt  Sounding temperature lines 220-160-000                10 Arial
skp  Sounding pressure lines    220-160-000                10 Arial
skd  Sounding dry adiabat lines 220-160-000                10 Arial
skw  Sounding wet adiabat lines 080-120-080                10 Arial
skm  Sounding mixing ratio lines080-120-080                10 Arial
szt  Sounding temperature text  147-106-000                10 Arial
szp  Sounding pressure text     155-113-000                10 Arial BOLD
szd  Sounding dry adiabat text  140-102-000                10 Arial
szw  Sounding wet adiabat text  080-120-080                10 Arial
szm  Sounding mixing ratio text 080-120-080                10 Arial
                                   -   -                      
                                   -   -                      
                                   -   -                      
                                   -   -                      
                                   -   -                      
                                   -   -                      
                                   -   -                      
                                   -   -                      
